;	SERWPL.INF - INF file for USB-to-Serial Device
;	Copyright (C) 1999, Prolific Technology Inc.
;
;	09/13/2000
[Manufacturer]
%MfgName%=Pro

[Pro]
%DeviceDesc%=ComPort, USB\VID_067B&PID_2303

[SourceDisksNames]
1="USB-Serial Cable Diskette",,,

[SourceDisksFiles]
SER9PL.SYS=1
SERSPL.VXD=1
SERSPL.INF=1
SERWPL.INF=1

[SourceDisksFiles.x86]
ser2pl.sys=1

[DestinationDirs]
USB2SER.Files.Ext = 11
USB2SER.Files.Inf = 10,INF
ComPort.NT.Copy = 12        ;DIRID_DRIVERS
SerialEnumerator.NT.Copy=12 ;DIRID_DRIVERS
NonPort.NT.Copy = 12        ;DIRID_DRIVERS

[ComPort_install]
;Windows98_ME

[Version]
Signature="$Chicago$"
Class=USB
provider=%Mfg%
LayoutFile=layout.inf
; DriverVer=8/15/2003,2.0.0.10

[PreCopySection]
HKR,,NoSetupUI,,1

[ComPort]
CopyFiles=USB2SER.Files.Ext, USB2SER.Files.Inf
AddReg=USB2SER.AddReg

[USB2SER.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,SER9PL.SYS

[USB2SER.Files.Ext]
SER9PL.SYS
SERSPL.VXD

[USB2SER.Files.Inf]
SERWPL.INF
SERSPL.INF

;========================================================================
;
;========================================================================
[ComPort_Install.NTx86]
;Windows2000

[Version]
Signature="$Chicago$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%Mfg%
LayoutFile=layout.inf
DriverVer=03/05/2004,2.0.0.25

AddReg=PortsClass.AddReg

[PortsClass.AddReg]
HKR,,,,%PortsClassName%

[ComPort.NT]
CopyFiles=ComPort.NT.Copy
AddReg=ComPort.AddReg, ComPort.NT.AddReg
; LogConfig=c14,c1a,c23,c2a,c34,c3a,c43,c4a,caa
LogConfig=c3a,c4a,caa
SyssetupPnPFlags = 1

[ClassInstall32.NT]
AddReg=PortsClass.NT.AddReg

[PortsClass.NT.AddReg]
HKR,,,,%PortsClassName%
HKR,,Icon,,"-23"
HKR,,Installer32,,"MsPorts.Dll,PortsClassInstaller"



[ComPort.NT.HW]
AddReg=ComPort.NT.HW.AddReg

[ComPort.NT.Copy]
ser2pl.sys

[ComPort.NT.AddReg]
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"
; Uncomment the following line if you want to override the advanced dialog for
; your device.  See msports.h for protoype of OverrideAdvancedFunction
; HKR,,EnumAdvancedDialog,,"yourdll.dll,OverrideAdvancedFunction"

[ComPort.NT.HW.AddReg]
HKR,,"UpperFilters",0x00010000,"serenum"

; MultiPort COM Sections;
; -------------------------------------------------------

[MultiComPort.NT]
CopyFiles=ComPort.NT.Copy
AddReg=ComPort.AddReg, ComPort.NT.AddReg
LogConfig=cm1,cm2,cm3,cm4,dg1,dga,cma
SyssetupPnPFlags = 1

[MultiComPort.NT.HW]
; Add multiport and normal port into the hardware devnode
AddReg=MultiComPort.NT.HW.AddReg,ComPort.NT.HW.AddReg

[MultiComPort.NT.HW.AddReg]
; Add multiport specific info to the hardware devnode
HKR,,MultiportDevice,0x00010001,1

; The serial enumerator by itself, so that other INFs can install serenum w/out ser2pl.sys
; -------------------------------------------------------

[SerialEnumerator.NT]
CopyFiles=SerialEnumerator.NT.Copy

[SerialEnumerator.NT.Copy]
serenum.sys

;-------------- Service installation
; Port Driver (function driver for this device)
[ComPort.NT.Services]
AddService = Ser2pl, 0x00000002, Serial_Service_Inst, Serial_EventLog_Inst
AddService = Serenum,,Serenum_Service_Inst

[MultiComPort.NT.Services]
AddService = Ser2pl, 0x00000002, Serial_Service_Inst, Serial_EventLog_Inst
AddService = Serenum,,Serenum_Service_Inst

[SerialEnumerator.NT.Services]
AddService = Serenum,,Serenum_Service_Inst

; -------------- Serial Port Driver install sections
[Serial_Service_Inst]
DisplayName    = %Serial.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_SYSTEM_START (this driver may do detection)
ErrorControl   = 1               ; SERVICE_ERROR_IGNORE
ServiceBinary  = %12%\ser2pl.sys
; LoadOrderGroup = Extended base

; -------------- Serenum Driver install section
[Serenum_Service_Inst]
DisplayName    = %Serenum.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\serenum.sys
LoadOrderGroup = PNP Filter

[Serial_EventLog_Inst]
AddReg = Serial_EventLog_AddReg

[Serial_EventLog_AddReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\ser2pl.sys"
HKR,,TypesSupported,0x00010001,7

[*pnp0500.det]
AddReg=Ports.AddReg,DevMap.AddReg

; The following sections are COM port resource configs.
; Section name format means:
; Char 1 = c (COM port)
; Char 2 = I/O config: 1 (3f8), 2 (2f8), 3 (3e8), 4 (2e8), a (any)
; Char 3 = IRQ config: #, a (any)

[c14]                   ; COM1,IRQ4
ConfigPriority=HARDRECONFIG
IOConfig=3f8-3ff(3ff::)
IRQConfig=S:4

[c1a]                   ; COM1, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=3f8-3ff(3ff::)
IRQConfig=S:3,4,5,7,9,10,11,12,14,15

[c23]                   ; COM2, IRQ3
ConfigPriority=HARDRECONFIG
IOConfig=2f8-2ff(3ff::)
IRQConfig=S:3

[c2a]                   ; COM2, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=2f8-2ff(3ff::)
IRQConfig=S:3,4,5,7,9,10,11,12,14,15

[c34]                   ; COM3, IRQ4
ConfigPriority=HARDRECONFIG
IOConfig=3e8-3ef(3ff::)
IRQConfig=S:4

[c3a]                   ; COM3, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=3e8-3ef(3ff::)
IRQConfig=S:3,4,5,7,9,10,11,12,14,15

[c43]                   ; COM4, IRQ3
ConfigPriority=HARDRECONFIG
IOConfig=2e8-2ef(3ff::)
IRQConfig=S:3,5

[c4a]                   ; COM4, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=2e8-2ef(3ff::)
IRQConfig=S:3,4,5,7,9,10,11,12,14,15

[caa]                   ; Any base, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=8@100-ffff%fff8(3ff::)
IRQConfig=S:3,4,5,7,9,10,11,12,14,15

; The following are multiport configs for DigiBoard (dgxx)
; and Comtrol (cmxx) multiport boards
; Section name format means:
; Char 1,2 = manufacturer abbreviation
; Char 3   = config number, a = no idea, use base setting

[cm1]
ConfigPriority=HARDRECONFIG
IOConfig=7@240-27E%3F8(3FF::)
IOConfig=247-247(3FF::)
IRQConfig=S:2,3,4,5,7,10,11

[cm2]
ConfigPriority=HARDRECONFIG
IOConfig=7@280-2BE%3F8(3FF::)
IOConfig=287-287(3FF::)
IRQConfig=S:2,3,4,5,7,10,11

[cm3]
ConfigPriority=HARDRECONFIG
IOConfig=7@500-5BE%FF8(3FF::)
IOConfig=507-507(FFF::)
IRQConfig=S:2,3,4,5,7,10,11

[cm4]
ConfigPriority=HARDRECONFIG
IOConfig=7@580-5BE%FF8(3FF::)
IOConfig=587-587(3FF::)
IRQConfig=S:2,3,4,5,7,10,11

[cma]
ConfigPriority=HARDRECONFIG
IOConfig=7@100-3FF%3F8(3FF::) ; I suspect we still need alignment here?
IOConfig=1@100-3FF(3FF::)     ; How about here?
IRQConfig=S:2,3,4,5,7,10,11

[dg1]
ConfigPriority=HARDRECONFIG
IOConfig=7@100-17E%3F8(3FF::)
IOConfig=140-140(3FF::)
IRQConfig=S:3,4,5,6,7,9,10,11,12,14,15

[dga]
ConfigPriority=HARDRECONFIG
IOConfig=7@100-3FF%3F8(3FF::) ; I suspect we still need alignment here?
IOConfig=1@100-3FF(3FF::)     ; How about here?
IRQConfig=S:3,4,5,6,7,9,10,11,12,14,15

; End COM port LogConfig sections



[ComPort.PosDup]
*PNP0500,*PNP0501,*PNP0502

[ComPort.NT.PosDup]
*PNP0500,*PNP0501,*PNP0502,*PNP0510,*PNP0511,*SMCF010

[DevMap.AddReg]
HKLM,hardware\devicemap\serialcomm,COM1,,COM1
HKLM,hardware\devicemap\serialcomm,COM2,,COM2


; "NoDrv" section: We do not yet support these port devices.
;----------------------------------------------------------
[NoDrv]

; "Non-port" sections: PCMCIA cards that look like COM
; ports, but aren't (excluding modems).
;----------------------------------------------------------
[NonPort]
CopyFiles=NonPort.Copy
AddReg=NonPort.AddReg

[NonPort.Copy]
serial.vxd

[NonPort.AddReg]
HKR,,PortSubClass,1,01
HKR,,DevLoader,,*vcomm
HKR,,PortDriver,,serial.vxd
HKR,,Contention,,*vcd
HKR,,DCB,3,1C,00,00,00, 80,25,00,00, 11,33,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00

[NonPort.NT]
;
; BUGBUG--Unclear whether these devices are presently supported under NT.  For now, leave a blank
; install section so we won't run the Win9x stuff.  The fact that no function driver will be installed
; for this devnode will cause the installation to fail, which is what we want to have happen for now.
;

; User readable strings
;----------------------------------------------------------
[Strings]
Mfg= "Prolific"
MfgName = "Prolific Technology Inc."
PortsClassName = "Ports (COM & LPT)"
DeviceDesc="Prolific USB-to-Serial Bridge"
Serial.SVCDESC   = "Prolific Serial port driver"
Serenum.SVCDESC = "Serenum Filter Driver"
